{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["行健特钢滚光矫直机技术参数"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"行健特钢滚光矫直机技术参数","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"merged":[[0,0,0,13],[1,0,2,0],[1,4,2,4],[1,5,2,5],[1,8,1,10]],"flags":["formulas_cached_only"]}
["矫直机技术参数"]
["型号","原料直径","原料","原料","辊轮个数","辊轮直径","辊轮转速","走料速度","成品精度",null,null,"主电机功率","升降电机功率","外型尺寸"]
[null,"(mm)","最大长度(m)","最小长度(m)",null,null,"无级变速","无级变速","直径公差","表面粗糙度","直线度","(KW)","(KW)","(m×m×m)"]
["JY15","Φ2.5～Φ15","不限",2,2,"Φ150mm","247～483r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.5mm/m","7.5×2",1.5,"5.0×1.3×1.4"]
["JY20","Φ4～Φ20","不限",1,2,"Φ180mm","10～80r/min","0～20m/min","≦h10","Ra≦0.4μm","0.15mm/m","7.5×2",1.5,"5.0×1.3×1.4"]
["JY40","Φ6～Φ40","不限",1,2,"Φ200mm","10～80 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.15mm/m","22×2",1.5,"5.5×1.4×1.5"]
["JY60","Φ12～Φ60","不限",1,2,"Φ250mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.15mm/m","30×2",3,"6.7×2.4×1.7"]
["JY80","Φ16～Φ80","不限",2,2,"Φ335mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.15mm/m","45×2",3,"8.7×3.4×3.3"]
["JY100","Φ16～Φ100","不限",2,2,"Φ360mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.2mm/m","55×2",3,"8.7×3.6×3.5"]
["JY120","Φ20～Φ120","不限",2,2,"Φ406mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.2mm/m","75 ×2",3.7,"9.8×4.5×4"]
["JY150","Φ40～Φ150","不限",2,2,"Φ530mm","5～30 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.5mm/m","132×2",7.5,"10.5×5×4.5"]
["JY200","Φ35～Φ200","不限",2.5,2,"Φ590mm","0～30 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.5mm/m","200×2",7.5,"11×6×6"]
["JY15A","Φ2.5～Φ15","不限",1,2,"Φ150mm","247～483r/min","0～30 m/min","≦h10","Ra≦0.6μm","0.5mm/m","7.5×2",0.12,"5.0×1.3×1.4"]
["JY20A","Φ4～Φ20","不限",1,2,"Φ180mm","10～80r/min","0～20m/min","≦h10","Ra≦0.4μm","0.15mm/m","7.5×2",1.5,"5.0×1.3×1.4"]
["JY40A","Φ6～Φ40","不限",1,2,"Φ200mm","10～80 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.5mm/m","22×2",2.2,"5.5×1.4×1.5"]
["JY60A","Φ12～Φ60","不限",1,2,"Φ250mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.15mm/m","30×2",3,"6.7×2.4×1.7"]
["JY80A","Φ16～Φ80","不限",2,2,"Φ335mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.15mm/m","45×2",3,"8.7×3.4×3.3"]
["JY100A","Φ16～Φ100","不限",2,2,"Φ360mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.2mm/m","55×2",3,"8.7×3.6×3.5"]
["JY120A","Φ20～Φ120","不限",2,2,"Φ406mm","10～50 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.2mm/m","75 ×2",3.7,"9.8×4.5×4"]
["JY150A","Φ40～Φ150","不限",2,2,"Φ570mm","5～30 r/min","0～30 m/min","≦h10","Ra≦0.4μm","0.5mm/m","132×2",7.5,"10.5×5×4.5"]
["JY200A","Φ35～Φ200","不限",2.5,2,"Φ590mm","0～30 r/min","0～30 m/min","≦h10","Ra≦0.4μm","2mm/m","200×2",7.5,"11×6×5"]